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Switch Wiring Diagram for 10 Pin Switch

Switch Circuit Pin - Tab Outs
7 uamton
7-Neg (- for
4 Fustroms upper light
5 cueme | 87 POS (+) for upper
light
6 cweveiow |1 - Outgoing
9 Qo) 2- Incoming
3- Outgoing
Lamp Circuit Wiring
8 7 4- Outgoing
5-Incoming
6- Outgoing
10 - Pos (+) for lower
light
10 4 9~ Neg (-) for lower
light
Notes

This is a dual lighted switch. Both lights in this switch are
wired to be independent of the switch operation.

If making your own harness:
Attach Both (White / Black Stripe) Wires together





