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Excessive Sulfur Odor

Service Category

Engine/Hybrid System

Section
Intake/Exhaust 

Market
USA 


Applicability

TSB SUPERSESSION NOTICE 

The information contained in this TSB supersedes TSB No. EG005-06.

^

Applicability has been updated to include 2007 - 2009 model year 4Runner vehicles. 

TSB No. EG005-06 is Obsolete and any printed versions should be discarded. Be sure to review the entire content of this service bulletin before proceeding.

Introduction

Some customers may complain of excessive sulfur odor on 2006 - 2009 model year 4Runner vehicles equipped with the 2UZ-FE engine under the following conditions:

^

Stop and go driving 

^

Heavy acceleration 

In order to reduce the sulfur odor new catalytic converter assemblies have been made available. Follow the repair procedure to replace the catalytic converter assemblies.

For more complete understanding of the root cause, refer to TSB No. EG003-03, "Sulfur Odor from Exhaust."
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   Warranty Information

APPLICABLE WARRANTY

^

This repair is covered under the Toyota Specified Major Emission Control Component Warranty. This warranty is in effect for 96 months or 80,000 miles, whichever occurs first, from the vehicle's in-service date. 

^

Warranty application is limited to occurrence of the specified condition described in this bulletin. 

[image: image2.png]1741050450

T7410-50490

Pipe Assembly Exhaust, Fron

745050121

T7450.50131

Pipe Assembly, Exhaust Fron, No_2





   




