PROGRAMMING ADDITIONAL or REPLACEMENT TRANSMITTERS

Each SECURIKEY+ system can be operated by up to four (4) different  SECURIKEY+ transmitters. The system is supplied from the factory with two (2) transmitters included, and additional transmitters are available through 
parts distribution. Any new or replacement transmitters will need to be programmed to the main control module before they will activate the system.  The SECURIKEY+ main control module uses a six (6) channel radio frequency receiver; each channel controlling a different function of the SECURIKEY+ system. Each transmitter button can be programmed to only one of the receiver channels (e.g., the GREEN button cannot be programmed to operate the headlight feature and remote start option; it can operate only one or the other feature). The following is a list of each receiver channel, and the function of each channel. 

CHANNEL # FEATURE CONTROLLED BY THIS CHANNEL 
1 Lock 
2 Unlock 
3 Trunk Release (optional kit required; not available on all models) 
4 30 second headlight activation (only if required by GREEN button) 
5 Remote panic (only if required by GREEN button instead of LOCK 
button) 
6 Remote start (optional kit required; not available on all models) 

To program new or additional transmitters, or when adding options to existing SECURIKEY+ transmitters, follow the step by step programming instructions found below. When programming, it is important to complete each 
step of the procedure within 15 seconds, or the system will terminate the programming mode. If this happens, simply start again. 

Be sure that the SECURIKEY+ system is disarmed, and the lighted valet switch is in the off (out) position before you begin. 
Turn the vehicle's ignition key to the on position. 
Press then release the L.E.D. valet switch 6 times. 

CHANNEL 1: LOCK & Panic Feature 
Horn Chirps 1 Time 
L.E.D. Flashes 1 Time 

To program the LOCK button on the transmitter, press and hold the LOCK button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the LOCK button programmed (up to four transmitters). 
After the LOCK button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to the next receiver channel. 


CHANNEL 2: UNLOCK Feature 
Horn Chirps 2 Times 
L.E.D. Flashes 2 Times 
To program the UNLOCK button on the transmitter, press and hold the UNLOCK 
button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the UNLOCK button programmed (up to four transmitters). 
After the UNLOCK button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to the next receiver channel. 

CHANNEL 3: TRUNK RELEASE 
Option Horn Chirps 3 
Times L.E.D. Flashes 3 Times
To program the TRUNK RELEASE option on the transmitter, press and hold the GREEN option button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the GREEN option button programmed (up to four transmitters). 
After the TRUNK RELEASE button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to the next receiver channel. 

CHANNEL 4: 30 SECOND HEADLIGHT Feature 
Horn Chirps 4 Times
 L.E.D. Flashes 4 Times
To program the HEADLIGHT option on the transmitter, press and hold the GREEN option button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the GREEN option button programmed (up to four transmitters). 
After the HEADLIGHT button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to the next receiver channel. 

CHANNEL 5: Separate PANIC Button Feature
 Horn Chirps 5 Times
 L.E.D. Flashes 5 Times 
To program the PANIC option on the transmitter, press and hold the GREEN option button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the GREEN option button programmed (up to four transmitters). 
After the PANIC button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to the next receiver channel. 


CHANNEL 6: REMOTE START Feature 
Horn Chirps 6 Times 
L.E.D. Flashes 6 Times
To program the REMOTE START option on the transmitter, press and hold the GREEN option button until the vehicle's horn sounds one loud chirp. Repeat this for all transmitters that need the GREEN option button programmed (up to four transmitters). 
After the REMOTE START button on all transmitters have been programmed, press and release the L.E.D. valet switch 2 times to advance to terminate programming mode, or simply turn the ignition key to the off position to 
terminate the transmitter programming mode. 

PROGRAMMING THE SELECTABLE FEATURES 
The SECURIKEY+ system offers a number of selectable features that can be changed, allowing you to custom fit the system to your customer. The following is a list of the features that are selectable and can be changed using the valet switch and any transmitter that is programmed to the system installed in the vehicle. 

FEATURE # FUNCTION 1 CHIRP 2 CHIRPS 
1 Headlights on for 20 seconds during disarm ON or OFF 
2 Headlights on for 20 seconds during arm ON or OFF 
3 Automatic ignition controlled door lock ON or OFF 
4 Automatic ignition controlled door unlock ON or OFF 
5 Auto unlock driver's door only or all doors Driver's door or All doors 
6 Active or Passive arming Passive or Active 
7 Active or Passive door locks Passive or Active 
8 Trunk release output - 1 second or latched 1 second or Latched 
9 Panic on lock button or option button Option or Lock 
10 Trunk Release Hold - 1 second or 2 presses Hold 1 Sec or 2 Times 

To change the selection of any of these features, follow the step by step programming procedures, and do not allow more then 15 seconds to pass between any two steps or the system will terminate the programming mode.  There is no need to complete the entire programming sequence. After the appropriate features have been changed, simply turn the ignition key off to terminate the programming mode. 

Be sure that the SECURIKEY+ system is disarmed, and the lighted valet switch is in the off (out) position before you begin. 
Turn the vehicle's ignition key to the on position. 
Press then release the L.E.D. valet switch 6 times. 
Immediately turn the ignition key off then back on. 

FEATURE 1 
LED Flashes 1 Time 
1 Chirp = Headlights ON During Disarm Horn Chirps either 1 or 2 Times 
2 Chirps = Headlights OFF During Disarm 
To change the selection, press and release the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and 
release the L.E.D. valet switch 2 times to advance to programmable feature number 2. 

FEATURE 2 
LED Flashes 2 Times 
1 Chirp = Headlights ON During Arm Horn Chirps either 1 or 2 Times 
2 Chirps = Headlights OFF During Arm 
To change the selection, press and release the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and 
release the L.E.D. valet switch 2 times to advance to programmable feature number 3. 

FEATURE 3 
LED Flashes 3 Times 
1 Chirp = Ignition controlled door locks ON Horn Chirps either 1 or 2 Times 
2 Chirps = Ignition controlled door locks OFF 
To change the selection, press and release the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. valet switch 2 times to advance to programmable feature number 4. 

FEATURE 4 
LED Flashes 4 Times 
1 Chirp = Ignition controlled unlock ON Horn Chirps either 1 or 2 Times 
2 Chirps = Ignition controlled unlock OFF 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to advance to programmable feature number 5. 


FEATURE 5 
LED Flashes 5 Times 
1 Chirp = Ignition controlled unlock DRIVER'S DOOR Horn Chirps either 1 or 2 Times 
2 Chirps = Ignition controlled unlock ALL DOORS 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to advance to programmable feature number 6. 

FEATURE 6 
LED Flashes 6 Times
1 Chirp = PASSIVE ARMING (Automatic Arming) Horn Chirps either 1 or 2 Times 
2 Chirps = ACTIVE ARMING (Arm by Remote Only) 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to advance to programmable feature number 7. 

FEATURE 7 
LED Flashes 7 Times 
1 Chirp = PASSIVE DOOR LOCKS Horn Chirps either 1 or 2 Times 
2 Chirps = ACTIVE DOOR LOCKS 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to advance to programmable feature number 8. 

FEATURE 8 
Do not change this feature selection. It should be left in the 
factory preset (1 chirp) mode. Press and release the L.E.D. valet switch 2 
times to advance to programmable feature 9. 

FEATURE 9 
LED Flashes 9 Times 
1 Chirp = Remote Panic / GREEN transmitter button Horn Chirps either 1 or 2 Times 
2 Chirps = Remote Panic / LOCK transmitter button 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to advance to programmable feature number 10. 

FEATURE 10 
LED Flashes 10 Times 
1 Chirp = Trunk Release HOLD GREEN BUTTON 1 SECOND Horn Chirps either 1 or 2 Times 
2 Chirps = Trunk Release PRESS GREEN BUTTON 2 TIMES 
To change the selection, press the lock button on the transmitter, which will be indicated by the appropriate 1 or 2 chirp signal from the horn. If you do not want to change this feature, simply press and release the L.E.D. 
valet switch 2 times to exit the programming mode.
