Caution: Any time when working on a vehicle raised off the ground it is necessary to secure the vehicle with jackstands to ensure safe working around the vehicle.
1. Jack up front end of truck and securely fasten with jackstands. I recommend lifting the whole front end, both sides of the truck off the ground, since otherwise the sway bar may make parts of the install more difficult. 

2. Remove wheels 

3. Remove lower shock mount nut 

4. Have a 2nd person apply downward pressure to the upper a-arm and use a hammer and punch to push lower shock mount bolt out of mount 

5. Caution: once the upper coil assembly mounting bolts are loosed coil assembly may fall out of mounting, so hold assembly while loosening these bolts Carefully remove upper coil assembly mounting bolts (3) 

6. Caution: when working with coil compressor ensure that compressors are securely in place and will not slip as coil could slip and spring out with considerable force. Install the coil compressor assembly onto coils and compress until coils are free to move between the upper shock plate and the shock itself. 

7. On the top portion of the shock is the nut that holds the whole assembly together. It may be necessary to hold the shock shaft so that it doesn’t turn as you loosen the nut. 

8. Once the whole assembly is disassembled take the top plate and carefully pull the rubber coil-centering piece off of the top plate. 
9. Install the rubber coil-centering piece from the stock top plate onto the spacer, and install the spacer into coilpack. 

10. Compress the coils tighter, to the point that you can fit the entire new assembly onto the shock.(this will either require a lot of patience with a ratchet or and impact wrench…recommend the impact if one is available) 

11. Once coils are tight enough to install complete the assembly, place all components back together, re-install upper shock mount bushings, and fasten the upper portion of the shock to the Spacer. 

12. Align two of the top mounting bolts parallel to the lower mounting centerline for alignment of assembly during re-installation. 

14. Re-install assembly, fastening top 3 mounting bolts first and securely fasten. 

15. Have a 2nd person hold pressure on the upper a-arm and re-install the lower shockmount bolt and securely fasten. 

16. Remount wheels and securely fasten and enjoy your new higher ride height Toyota Truck!
17. Remember a front-end alignment is needed to correct alignment adjustments or treadwear will occur. 

Warnings
Installation of a spacer lift may increase the risk of a rollover in some driving situations. These spacers are designed to create a mild lift to increase ground clearance and fenderwell clearance for the use of larger tires for offroad purposes. The user assumes all liability for any damage to vehicle due to negligent driving. Remember that these spacers don’t re-inforce the frame or other related suspension components. Enjoy your new spacer lift, but also operate your vehicle responsibly and you will enjoy many years of 4x4ing in your lifted Toyota. It is recommended that owner should get a front-end alignment after installing these spacer as they may require readjustment of some front end components. 
